# TTGO-TM-ESP32

## Website

### ESP_IDF:https://github.com/espressif/esp-idf



## Bluetooth audio

### DEMO:https://github.com/kodera2t/ESP32_OLED_webradio

![image](https://github.com/LilyGO/TTGO-TM-ESP32/blob/master/Image/image1.jpg)

### 1.Note that Data pin 22 is changed to pin 19.
      ESP32_OLED_webradio/components/audio_renderer/audio_renderer
      ![image](https://github.com/LilyGO/TTGO-TM-ESP32/blob/master/Image/Image8.png)
### 2.make menuconfig
      open buletooth
      ![image](https://github.com/LilyGO/TTGO-TM-ESP32/blob/master/Image/Image9.png)
      ![image](https://github.com/LilyGO/TTGO-TM-ESP32/blob/master/Image/Image10.png)
      ![image](https://github.com/LilyGO/TTGO-TM-ESP32/blob/master/Image/Image11.png)
      ![image](https://github.com/LilyGO/TTGO-TM-ESP32/blob/master/Image/Image12.png)
      ![image](https://github.com/LilyGO/TTGO-TM-ESP32/blob/master/Image/Image13.png)
### 3.make all && make flash

### In order to prevent accidents, the completion of the compiler above can be directly programmed. Of course, DIY will be more fun

## Album clock

### DEMO:https://github.com/moononournation/ESP32_BiJin_ToKei

![image](https://github.com/LilyGO/TTGO-TM-ESP32/blob/master/Image/image2.jpg)


![image](https://github.com/LilyGO/TTGO-TM-ESP32/blob/master/Image/image3.jpg)

![image](https://github.com/LilyGO/TTGO-TM-ESP32/blob/master/Image/image4.jpg)
